**City of Oviedo Fire Rescue**

**Monthly SCBA Check-off**

Date: \_\_\_\_\_ / \_\_\_\_\_ / \_\_\_\_\_ Unit # SCBA Pack #

Person Inspecting SCBA (PRINT):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | |  | **PASS** |  | **FAIL** |
| **MAIN FRAME** | |  |  |  |  |
|  | Frame inspected for dents, gouges, & other signs of damage |  |  |  |  |
|  | Hoses inspected for rips, tears, & cracks |  |  |  |  |
|  | Quick connect fittings operate appropriately |  |  |  |  |
|  | Straps & buckles inspected for damage and operate appropriately |  |  |  |  |
|  |  |  |  |  |  |
| **REGULATOR** | |  |  |  |  |
|  | Regulator inspected for dents, gouges, & other signs of damage |  |  |  |  |
|  | Heads-up display shows correct air supply level |  |  |  |  |
|  | Vibralert alarm activates when SCBA is turned on |  |  |  |  |
|  | Bypass (Purge) valve operates appropriately |  |  |  |  |
|  |  |  |  |  |  |
| **REMOTE GAUGE** | |  |  |  |  |
|  | Remote gauge inspected for dents, gouges, & other signs of damage |  |  |  |  |
|  | Remote gauge reads the same as the cylinder |  |  |  |  |
|  | Manual PASS activation functions appropriately |  |  |  |  |
|  |  |  |  |  |  |
| **BOTTLE** | |  |  |  |  |
|  | Cylinder inspected for dents, gouges, & other signs of damage |  |  |  |  |
|  | Ensure latest hydrostatic test date is current |  |  |  |  |
|  | Cylinder pressure gauge is operable and reads 4500 psi |  |  |  |  |
|  | Cylinder valve hand wheel operates appropriately |  |  |  |  |
|  |  |  |  |  |  |
| **PASS** | |  |  |  |  |
|  | PASS device activates when SCBA bottle is turned on |  |  |  |  |
|  | PASS alarm activates when pack is stationary |  |  |  |  |
|  | Manual PASS activation functions appropriately |  |  |  |  |
|  |  |  |  |  |  |
| **MASK (Spare mask)** | |  |  |  |  |
|  | Mask inspected for rips, cracks, and other damage |  |  |  |  |
|  | Head harness inspected for rips, tears, & missing parts |  |  |  |  |
|  | Nose cup inspected for rips, tears, & cracks |  |  |  |  |

If damage is noted to the SCBA or its components, remove it from service and notify the SCBA Coordinator via the Chain of Command for repairs. Replacement SCBA packs can be located at