# City of Oviedo Fire Rescue Stretcher Check-off

Date: / / Unit # Stretcher Serial #

Person Inspecting Stretcher (PRINT):

# BACK REST YES NO

Operable

Bent or Broken Tubing Loose or Missing Parts

# MAIN FRAME

Missing or Loose Pins Bent or Broken Tubing Missing or Loose Bolts Side Arms Operable Operates in all Positions

# LOWER FRAME

Cracks in Welds Missing or Loose Pins Bent or Broken Tubing Worn Scuff Marks

# WHEELS

Proper Tread Loose Bolts

Loose Wheel Mounts

# TRENDELENBERG

Operable

Bent/Broken Tubing or Support Bars Loose or Missing Pins

# MATTRESS

Cracks Tears Holes

**POWER LOAD – If Applicable** Power Load Serial # Operable

Missing/Loose Bolts Track Slides Easily Battery Charges

Manual Override Operable

Any operations should be smooth and easy to accomplish, if they are not notify the EMS Coordinator via the Chain of Command.

Any time a patient is transported that exceeds the manufacturer’s recommended weight limit for the stretcher, notify the EMS Coordinator via the Chain of Command so a re-inspection by the EMS Coordinator or his/her designee can be performed.